For 1990-2009 cars

### Removal Procedure

1. Remove the spare tire and wheel assembly from the spare wheel carrier.
2. Gently pull the rear window washer nozzle (1) from the rear window washer nozzle mounting hole (3) below the rear door window.
3. Disconnect the rear window washer nozzle hose (2) from the rear window washer nozzle (1).
4. Remove the rear window washer nozzle (1) from the vehicle.

### Installation Procedure

1. Connect the rear window washer nozzle hose (2) to the rear window washer nozzle (1).
2. Install the rear window washer nozzle (1) to the rear window washer nozzle mounting hole (3) below the rear door window.
3. Install the spare tire and wheel assembly to the spare wheel carrier.