For 1990-2009 cars

1. Remove the speedometer drive gear retainer ring from the output shaft, if equipped.
2. Remove the speedometer drive gear retaining clip (339).
3. Remove the speedometer drive gear (340).

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the extension housing from the transmission case. Refer to Extension Housing Removal in this section.
3. Remove the 2 speedometer drive gear retaining rings (1) from the transmission output shaft (3).
4. Remove the speedometer drive gear (2).
5. Inspect the speedometer drive gear (2) for abnormal wear or damage. Replace the drive gear, if necessary.