For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door inside handle (1). Refer to Rear Side Door Inside Handle Replacement .
2. Remove the screw which secures the rear side door pull handle (3).
3. Use a cloth in order to pull off the snap ring which secures the rear side door window regulator handle (1), if equipped.
4. Remove the window regulator handle (1), if equipped.
5. Gently pry the rear side door trim panel (2) from the rear side door by disengaging the plastic retainers which secure the panel.
6. Position the door trim panel (2) away from the door in order to gain access to the rear side window switch electrical connector, if equipped.
7. Disconnect the window switch electrical connector, if equipped.
8. Remove the door trim panel (2) from the vehicle.
9. Remove the rear side window switch from the door trim panel (2) by releasing the 4 plastic retaining tabs, as needed.

### Installation Procedure

1. Install the rear side window switch to the rear side door trim panel (2), if removed. Ensure that the 4 plastic retaining tabs are fully engaged.
2. Connect the rear side window switch electrical connector, if equipped.
3. Install the door trim panel (2) to the rear side door. Ensure that the plastic retainers are fully engaged.
4. Install the rear side door window regulator handle snap ring (1) to the rear side door window regulator handle (2), if equipped.
5. Install the window regulator handle (2) to the door, if equipped.
6. Install the screw which secures the rear side door pull handle (3).
7. Install the rear side door inside handle (1). Refer to Rear Side Door Inside Handle Replacement .