For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Starting System Check performed? | -- | Go to Step 2 | Go to Starting System Check
2 |

1. Place the gear selector lever in neutral and depress the clutch (manual transmission).
2. Engage the parking brake and place the manual selector lever in P or N (automatic transmission).
3. Test for battery voltage at the starter solenoid terminal S with the ignition switch in the START position.

Is battery voltage present?

--

Go to Step 3

Go to Step 4

3 | Replace the starter solenoid. Refer to Starter Motor Overhaul . Is the repair complete? | -- | Go to Starting System Check | --
4 |

• | Test for battery voltage at terminal 3 of the transmission range switch (4 speed automatic transmission ) with the ignition switch in the START position.

• | Test for battery voltage at connector 1 terminal 2 of the park/neutral position (PNP) switch (3 speed automatic transmission ) with the ignition switch in the START position.

• | Test for battery voltage at terminal 2 of the clutch pedal position (CPP) switch with the clutch pedal depressed (manual transmission) and the ignition switch in the START position.

Is battery voltage present?

--

Go to Step 5

Go to Step 6

5 | Repair the open in the BLK/YEL wire between the transmission range, or PNP or CPP switch and the starter solenoid. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Starting System Check | --
6 |

• | Test for battery voltage at terminal 2 of the transmission range switch with the ignition switch in the START position.

• | Test for battery voltage at terminal 1 of the PNP switch with the ignition switch in the START position.

• | Test for battery voltage at terminal 1 of the CPP switch with the clutch pedal depressed and the ignition switch in the START position.

Is battery voltage present?

--

Go to Step 7

Go to Step 8

7 |

• | Replace the transmission range switch. Refer to Transmission Range Switch Replacement in Automatic Transmission.

• | Replace the CPP switch. Refer to Clutch Pedal Position Switch Replacement in Clutch.

Is the repair complete?

--

Go to Starting System Check

--

8 | Test for battery voltage at terminal 6 of the ignition switch connector with the ignition switch in the START position. Is battery voltage present? | -- | Go to Step 9 | Go to Step 10
9 | Repair the open in the BLK/RED wire between the ignition switch and the transmission range, PNP or CPP switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Starting System Check | --
10 | Test for battery voltage at terminal 5 of the ignition switch connector. Is battery voltage present? | -- | Go to Step 11 | Go to Step 12
11 | Replace the ignition switch. Refer to Ignition Switch Replacement - On Vehicle in Steering Wheel and Column-Standard. Is the repair complete? | -- | Go to Starting System Check | --
12 | Test for battery voltage at the fuse block connector 4 terminal 1. Is battery voltage present? | -- | Go to Step 13 | Go to Step 14
13 | Repair the open in the WHT/GRN wire between the fuse block connector 4 terminal 1 and the ignition switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Starting System Check | --
14 | Test for an open in the BLK wire between the battery and fuse block 1. Is an open present? | -- | Go to Step 16 | Go to Step 15
15 | Replace the fuse block. Is the repair complete? | -- | Go to Starting System Check | --
16 | Repair the open in the BLK wire between the battery and fuse block 1. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Starting System Check | --