For 1990-2009 cars

#### Tools Required

J 37228 Seal Cutter

1. Remove the left upper valve rocker arm cover screws.
2. Separate the upper valve rocker arm cover from the lower valve rocker arm cover using J 37228 .
3. Remove the left upper valve rocker arm cover.
4. Remove and discard the valve rocker arm cover gasket, valve rocker arm cover grommets and valve rocker arm cover bolts if they are serviced with the grommet.