For 1990-2009 cars

Problem | Action
--- | ---
The springs are broken or sagging. | Inspect and repair as necessary. Refer to Front Coil Springs Replacement in Front Suspension or Coil Spring Replacement in Rear Suspension.
The stabilizer shaft is loose or disconnected. | Inspect the stabilizer shaft links and insulators for damage. Repair or replace as necessary. For stabilizer shaft link replacement, Refer to Stabilizer Shaft Link Replacement in Front Suspension.
The vehicle is overloaded. | Reduce the vehicle load. Refer to Vehicle Certification Label in General Information.
The tire pressure(s) is incorrect. | Inflate the tire(s) to proper specifications. Refer to the tire placard on the driver's door lock pillar.