For 1990-2009 cars

### Removal Procedure

1. Remove the radiator grille. Refer to Grille Replacement .
2. Remove the following components from the radiator grille (1):

2.1. | The 5 screws (2)

2.2. | The radiator grille molding

### Installation Procedure

1. Install the radiator grille molding to the radiator grille (1). Secure the molding with the 5 screws (2).
2. Install the radiator grille. Refer to Grille Replacement .