For 1990-2009 cars

1. Move the steering wheel in the shaft direction in order to inspect for looseness or a rattle. If the steering wheel is loose or rattles, tighten or replace the steering wheel as necessary. Refer to Steering Wheel Replacement .
2. Move the steering wheel in a lateral direction in order to inspect for looseness. If the steering wheel is loose, tighten or replace the steering wheel as necessary. Refer to Steering Wheel Replacement .
3. With the engine OFF, the vehicle on level ground, and the front tires and wheels in a straight forward position, rotate the steering wheel to the left and to the right. Measure the steering wheel play.

Measurement
The steering wheel play tolerance is 0-30 mm (0-1.2 in).

4. If steering wheel play is not within specification, inspect the following components for looseness, wear, or damage.

• | The tie-rod end ball stud

• | The lower ball joint

• | The steering shaft coupling

• | The steering gear

5. Tighten loose components. Replace defective parts. Refer to the following procedures:

• | Rack and Pinion Outer Tie Rod End Replacement in Power Steering

• | Lower Control Arm Replacement in Front Suspension

• | Steering Shaft Coupling Replacement

• | Steering Gear Replacement in Power Steering