For 1990-2009 cars

### Circuit Description

Battery voltage is applied to the ignition coils when the ignition switch is turned to the ON or START positions. The ignition control module circuitry within the coil assemblies toggles the primary windings of the ignition coil in order to induce a high voltage in the secondary windings of the ignition coil. The powertrain control module (PCM) controls the ignition event based on numerous inputs including the crankshaft position sensor. The high voltage induced in the secondary windings of the ignition coils is applied through the spark plug wires and coil boots to the spark plugs.

In order for the engine to start and run the correct amount of good quality fuel must be properly delivered to each cylinder. The timing of the valve train operation in relation to piston position is also critical, as is the mechanical compression of the air/fuel mixture.

### Diagnostic Aids

Check for any of the following conditions:

• | Insufficient fuel can cause a no start condition. Thoroughly inspect the fuel delivery system for sufficient fuel volume to the fuel injectors. Inspect the fuel supply components for partial blockage or restrictions.

• | There may be fuel spray at the fuel injectors and the indicated fuel pressure may be correct, yet there may not be enough fuel to start the engine. If the fuel injectors and the injector circuit are OK, and fuel spray is detected, the fuel injector ON time may be inadequate. If the PCM receives incorrect inputs from the various information sensors, the fuel delivered by the fuel injectors may be inadequate to start the engine. Check all the engine data parameters with a scan tool and compare the values indicated with the expected values or the values from a known good vehicle.

• | Check the battery condition and the engine cranking speed. The engine will not start and improper diagnosis may occur if the starting system is not operating to necessary levels. Refer to Engine Cranks Slowly in Engine Electrical.

• | Water or foreign material can cause a no start during freezing weather. The engine may start after sitting in a heated garage. The malfunction may not recur until the vehicle is parked overnight in freezing temperatures.

• | The PCM relies on the CMP sensor for engine reference. Without continuous accurate reference signals, there is no reliable spark or fuel injector pulse. The scan tool engine speed display should be about 200 RPM while cranking. If erratic values, such as sudden spikes in engine speed are displayed, the engine reference signal may not be stable enough for the engine to start and run properly. Inspect the CMP sensor signal circuit for electromagnetic interference (EMI) or poor electrical connections.

• | A vehicle that starts and runs after being brought to the shop for an engine cranks but will not run complaint, may have an ignition system that is susceptible to moisture. Spray water on the ignition system components and wiring in order to check for an engine miss or stall.

• | A vehicle that starts and runs only when holding the accelerator pedal down slightly, may have a fault in the IAC system. Turn OFF the ignition and disconnect the idle air control (IAC) valve. If the engine will now start and stay running, refer to Idle Air Control (IAC) System Diagnosis .

• | Check for a malfunctioning main relay. Intermittent main relay operation can cause no MIL and an engine that cranks but will not run. Refer to Ignition Relay Diagnosis .

An intermittent malfunction may be caused by a problem in the ignition system electrical circuit. Inspect the wiring harness and components for an intermittent condition. Refer to Intermittent Conditions .

### Test Description

The numbers below refer to the step numbers in the diagnostic table.

1. The Diagnostic System Check-Engine Controls prompts the technician to complete some basic checks and stores the Freeze Frame data on the scan tool if applicable. This creates an electronic copy of the data taken when the fault occurred. The information is then stored in the scan tool for later reference.

2. The PCM relies on the CMP sensor for engine reference. Without engine reference signals there is no spark and no fuel injector pulse. A DTC P0340 sets after 3 seconds when cranking the engine if no CMP sensor signal is present.

3. This step checks the TP sensor, the ECT sensor, and the MAP sensor for a faulty signal. A faulty sensor input to the PCM may cause a fueling condition that results in a no start.

4. This step checks for adequate secondary ignition voltage at the spark plugs.

5. This step checks to see if fuel system pressure is within specifications with the ignition ON and the fuel pump running. The fuel pump may be operated with the scan tool Output Control feature when the fuel level is more than 20 percent.

6. Fouled or contaminated spark plugs indicate that another malfunction exists. If the engine starts and runs after cleaning or replacing the spark plugs, inspect for the cause of the spark plug condition. Road testing the vehicle and inspecting the vehicle performance with a scan tool can prevent a no start from reoccurring.

7. Fuel injectors with partially blocked and restricted nozzles, or a malfunctioning solenoid, can cause a no start condition. The fuel injector inspections can locate faulty injectors.

8. This step checks for proper resistance of the ignition coil secondary windings.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
Schematic Reference: Engine Controls Schematics
1 | Did you perform the Diagnostic System Check-Engine Controls? | -- | Go to Step 2 | Go to Diagnostic System Check - Engine Controls
2 | Check for DTCs with a scan tool. Is a DTC P0340 set? | -- | Go to DTC P0340 | Go to Step 3
3 |

1. Turn ON the ignition, leaving the engine OFF.
2. Check the scan tool data parameters of the following sensors:

• | Engine coolant temperature (ECT) sensor

• | Throttle position (TP) sensor

• | Manifold absolute pressure (MAP) sensor

3. Locate the cause of any sensor reading that is not within expected values.
4. Repair as necessary.

Was a repair necessary?

--

Go to Step 13

Go to Step 4

4 |

1. Disconnect the fuel injector electrical connectors.
2. Install a J 26792 spark tester or an equivalent to the #1 spark plug wire.
3. Check for spark while cranking the engine.
4. Remove the #1 ignition coil.
5. Re-install the spark plug wire.
6. Install the spark tester to the ignition coil boot.
7. Check for spark while cranking the engine.
8. Repeat steps 2 through 7 for the #2 ignition coil.

Did the test of each cylinder indicate a good crisp blue spark while cranking the engine?

--

Go to Step 5

Go to Electronic Ignition (EI) System Diagnosis

5 |

1. Turn OFF the ignition.
2. Install the J 34730-1A fuel pressure gauge or an equivalent. Refer to Fuel Pressure Gage Installation and Removal .

Important: In order to obtain maximum fuel pressure it may be necessary to cycle the ignition ON to OFF to ON more than once.

3. Turn ON the ignition, leaving the engine OFF. The fuel pump should run for approximately 2 seconds.
4. Observe the fuel pressure with the fuel pump running.

Is the fuel pressure indicated within the specified values?

250-300 kPa (36 to 43 psi)

Go to Step 7

Go to Step 6

6 |

1. Turn ON the ignition, leaving the engine OFF. The fuel pump should run for approximately 2 seconds.
2. Observe the fuel pressure.

Did the fuel pressure gauge indicate any pressure more than the specified value?

0.0-7.0 kPa (0 to 1.0 psi)

Go to Fuel System Diagnosis

Go to Fuel Pump Electrical Circuit Diagnosis

7 |

1. Collect a fuel sample.
2. Inspect a fuel sample for the following concerns:

• | Alcohol or other contamination, refer to Alcohol/Contaminants-in-Fuel Diagnosis .

• | The fuel type and quality

3. Replace the fuel as necessary. Refer to Fuel Tank Draining .

Was a fuel concern found and replaced?

--

Go to Step 13

Go to Step 8

8 |

1. Inspect the spark plugs for correct operation and condition. Refer to Spark Plug Inspection .
2. Clean or replace the spark plugs as necessary. Refer to Spark Plug Replacement .

Was a repair or replacement necessary?

--

Go to Step 13

Go to Step 9

9 |

1. Turn OFF the ignition.
2. Disconnect all four fuel injector electrical connectors.
3. Install a J 34730-2B injector test light or an equivalent into each fuel injector harness connector.
4. Observe the injector test lamp for each injector while cranking the engine.

Did the injector test lamp flash for each injector while cranking the engine?

--

Go to Step 10

Go to Fuel Injector Circuit Diagnosis

10 | Check for faulty fuel injectors. Refer to Fuel Injector Solenoid Coil Test - Engine Coolant Temperature Between 10-35 Degrees C (50-95 Degrees F) and Fuel Injector Balance Test with Special Tool . Did you find and replace a faulty fuel injector? | -- | Go to Step 13 | Go to Step 11
11 |

1. Inspect the exhaust system for blockage or a restriction. Refer to Restricted Exhaust in Engine Exhaust.
2. Repair or replace the exhaust system as necessary.

Was a restriction in the exhaust system found and repaired?

--

Go to Step 13

Go to Step 12

12 |

1. Check for any of the following engine mechanical conditions:

• | Worn or faulty camshaft

• | Leaking or sticking valves

• | Leaking or sticking piston rings

• | Excessive valve deposits

• | Collapsed or sticking lifters

• | Loose or worn rocker arms

• | Weak valve springs

• | Incorrect valve timing

• | Leaking head gasket

2. Repair as necessary. Refer to Engine Compression Test in Engine Mechanical.

Did you find and repair a basic engine mechanical problem?

--

Go to Step 13

Go to Diagnostic Aids

13 |

1. Perform the scan tool Clear DTC Information function.
2. Attempt to start the engine.

Does the engine start and continue to run?

--

Go to Step 14

Go to Step 2

14 |

1. Operate the engine at idle until a normal operating temperature is reached.
2. Check for DTCs with a scan tool.

Are any DTCs displayed?

--

Go to Diagnostic Trouble Code (DTC) List

Go to Step 15

15 | With the scan tool review the stored information, Capture Info. Does the scan tool display any DTCs that you have not diagnosed? | -- | Go to Diagnostic Trouble Code (DTC) List | System OK