For 1990-2009 cars

### Removal Procedure

1. Remove the rear folding top material. Refer to Folding Top Material Replacement .
2. Remove the following components from the vehicle:

2.1. | The 3 screws

2.2. | The folding top bow garnish molding (2)

### Installation Procedure

1. Install the folding top bow garnish molding (2) to the vehicle. Secure the molding with the 3 screws.
2. Install the rear folding top material. Refer to Folding Top Material Replacement .