For 1990-2009 cars

### Removal Procedure

1. Mark the position of the lock striker (1) on the rear door jamb.
2. Remove the 2 lock striker screws.
3. Remove the lock striker (1) from the rear door jamb.

### Installation Procedure

1. Install the lock striker (1) to the rear door jamb. Secure the lock striker (1) with the 2 screws.
2. Adjust the lock striker (1) vertical measurement in order to align with the center of the rear door lock assembly (2).
3. Keep the lock striker (1) level while moving the lock striker sideways in order to adjust the rear door flushness with the quarter panel, as needed. Refer to Door Adjustment Specifications in Doors.