For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Drum Inner Diameter (Maximum):

- 2-Door

222 mm

8.74 in

- 4-Door

256 mm

10.07 in

Drum Out-of-Round (Maximum) | 0.01 mm | 0.0004 in
Drum Roundness Runout (Maximum) | 0.04 mm | 0.0016 in
Drum Taper (Maximum) | 0.1 mm | 0.004 in
Linings Outer Diameter:

- 2-Door

219.4 mm

8.64 in

- 4-Door

253.5 mm

9.98 in

Shoe Lining Material Thickness (Minimum) | 1 mm | 0.04 in