For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Countershaft Rear Bearing Retaining Ring | 1.80 mm | 0.0709 in
Countershaft Rear Bearing Retaining Ring | 1.90 mm | 0.0748 in
Countershaft Rear Bearing Retaining Ring | 2.00 mm | 0.0787 in
Countershaft Rear Bearing Retaining Ring | 2.10 mm | 0.0827 in
4th/5th Gear Synchronizer Hub Retaining Ring | 2.00 mm | 0.0787 in
4th/5th Gear Synchronizer Hub Retaining Ring | 2.05 mm | 0.0807 in
4th/5th Gear Synchronizer Hub Retaining Ring | 2.10 mm | 0.0827 in
4th/5th Gear Synchronizer Hub Retaining Ring | 2.15 mm | 0.0846 in
4th/5th Gear Synchronizer Hub Retaining Ring | 2.20 mm | 0.0866 in
4th/5th Gear Synchronizer Hub Retaining Ring | 2.25 mm | 0.0886 in
4th/5th Gear Synchronizer Hub Retaining Ring | 2.30 mm | 0.0906 in
4th/5th Gear Synchronizer Hub Retaining Ring | 2.35 mm | 0.0925 in
4th/5th Gear Synchronizer Hub Retaining Ring | 2.40 mm | 0.0945 in
4th/5th Gear Synchronizer Hub Retaining Ring | 2.45 mm | 0.0965 in
4th/5th Gear Synchronizer Hub Retaining Ring | 2.50 mm | 0.0984 in