For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 1859-A Steering Wheel Puller

1. Disable the supplemental inflatable restraint (SIR). Refer to Disabling the SIR System in SIR.

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

2. Disconnect the negative battery cable.
3. Remove the steering wheel inflator module. Refer to Steering Wheel Inflator Module Replacement .
4. Remove the steering wheel retaining nut (1) from the shaft.
5. Scribe an alignment mark (1, 2) across the steering wheel and the steering shaft in order to ease the installation.
6. Install the J 1859-A Steering Wheel Puller to the steering wheel (1).
7. Remove the steering wheel (1) from the steering shaft.

### Installation Procedure

Important: When you install the steering wheel, the 2 lugs on the SIR coil must line up with the 2 grooves on the back side of the steering wheel. Turning the steering wheel can damage the SIR coil if the lugs do not line up with the grooves.

1. Match the alignment marks (1, 2) on the steering wheel and the steering shaft in order to install the steering wheel to the steering shaft.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Secure the steering wheel to the steering shaft with the steering wheel retaining nut.

Tighten
Tighten the steering wheel retaining nut to 33 N·m (24 lb ft).

3. Install the inflator module. Refer to Steering Wheel Inflator Module Replacement .
4. Connect the negative battery cable.
5. Enable the SIR. Refer to Enabling the SIR System in SIR.