For 1990-2009 cars

### Removal Procedure

1. Unfasten the corner flap of the rear folding top material on the lower left side of the rear door in order to uncover the zipper pull ring.
2. Unfasten the corner flap of the rear folding top material on the lower right side of the rear door.
3. Completely unzip the zipper from the rear folding top material.
4. Drape the folding top rear window down and rearward.
5. Pull the folding top rear window and the folding top rear window lower frame reinforcement rearward in order to remove the window and frame from the vehicle.
6. Slide the folding top rear window sideward in order to remove the window from the window lower frame reinforcement.
7. Place the rear window on a clean, flat surface with the inside facing up.

### Installation Procedure

1. Slide the folding top rear window sideward into the folding top rear window lower frame reinforcement.
2. Install the rear window and lower frame reinforcement to the vehicle.
3. Zip the rear window to the rear folding top material.
4. Fasten the rear folding top material corner flaps on the lower right and left sides of the rear window lower frame reinforcement.