For 1990-2009 cars

## Folding Top Material Replacement Front

### Removal Procedure

1. Lower the radio antenna.
2. Swing the sunshades down in order to gain access to the folding top latches (1).
3. Push in the folding top latch buttons (2).
4. Pull the latch (1) back.
5. Unhook the latch (1) from the front top bow.
6. Lift the front top bow.
7. Unsnap (1) the front folding top material (3) from the folding top #1 bow (4).
8. Unsnap the snap (3) which secures each tension strap (1).
9. Pull the straps (1) out of the plastic loops (2).
10. Unsnap (1) the front folding top material from the roof support (3), near the dome lamp.
11. Fold the front folding top material (1) back in order to gain access to the screws which secure the material to the front folding top weatherstrip retainer (3).
12. Remove the screw (2) from each side which secures the front folding top material (1) to the front folding top weatherstrip retainer (3).
13. Remove the front folding top material (1) from the vehicle.

### Installation Procedure

1. Install the front folding top material to the vehicle.
2. Install the screw (2) to each side which secures the front folding top material (1) to the front folding top weatherstrip retainer (3).
3. Position the front folding top material in order to snap (1) the material to the roof support (3), near the dome lamp.
4. Snap (1) the front folding top material (3) to the folding top #1 bow (4).
5. Pull the tension straps (1) through the plastic loops (2). Secure each strap by snapping the snap (3).
6. Hook the folding top #1 bow to the folding top latches (1).
7. Push the latches (1) down until the latches click into place.
8. Return the sunshades back to their original position.
9. Raise the radio antenna.

## Folding Top Material Replacement Rear

### Removal Procedure

1. Remove the folding top rear window. Refer to Folding Top Rear Window Replacement .
2. Remove the folding top quarter windows. Refer to Folding Top Quarter Window Replacement .
3. Unsnap (1) the front folding top material from the roof support (3), near the dome lamp.
4. Unsnap the rear folding top material (2) from the roof support (3), near the dome lamp.
5. Push down on the folding top #3 bow release button (1) on each side and tilt the base (2) of the #3 bow (3) forward. This will remove the tension from the rear folding top material.
6. Unsnap the rear folding top material from the folding top #3 bow (3).
7. Detach the rear bottom corners of the rear folding top material.
8. Detach the front of the rear folding top material (2) by unhooking from the folding top side body joint cover (1).
9. Remove the rear folding top material (2) from the vehicle.

### Installation Procedure

1. Install the rear folding top material (2) to the vehicle. Secure the material by attaching the front of the material to the folding top side body joint cover (1).
2. Install the rear folding top material (2) over the folding top #3 bow.
3. Fasten the rear bottom corners of the rear folding top material to the body.
4. Snap the rear folding top material to the folding top #3 bow.
5. Position the folding top #3 bow base (2) rearward and return the bow (3) to the upright position in order to apply tension to the folding top material.
6. Snap (1) the rear folding top material (2) to the roof support (3), near the dome lamp.
7. Snap (1) the front folding top material to the roof support (3), near the dome lamp.
8. Install the folding top quarter windows. Refer to Folding Top Quarter Window Replacement .
9. Install the folding top rear window. Refer to Folding Top Rear Window Replacement .