For 1990-2009 cars

### Removal Procedure

1. Remove the Knee bolster. Refer to Instrument Panel, Gages and Console.
2. Disconnect the EBCM (1) electrical connectors.
3. Remove the three retaining nuts and remove the EBCM from the mounting bracket.

### Installation Procedure

1. Install the EBCM (1) to the bracket. Secure the EBCM (1) with the three retaining nuts.
2. Install the three retaining nuts.

Tighten
Tighten the retaining nuts to 11 N·m (97 lb in).

3. Connect the EBCM electrical connectors.
4. Install the Knee bolster. Refer to Instrument Panel, Gages and Console.
5. Perform the Diagnostic System Check .