For 1990-2009 cars

### Removal Procedure

1. Remove the grille from the vehicle. Refer to Grille Replacement in Exterior Trim.
2. Turn the lock ring (4) counterclockwise in order to remove the headlamp bulb (3) from the headlamp assembly (2).
3. Remove the 4 screws from the headlamp assembly.
4. Remove the headlamp assembly (2) from the vehicle.
5. Remove the park/turn lamp bulb socket (3) from the park/turn lamp housing.
6. Remove the 3 screws from the park/turn lamp housing (3).
7. Remove the housing (3) from the headlamp assembly mounting bracket (1).

### Installation Procedure

1. Install the park/turn lamp housing (3) to the headlamp assembly mounting bracket (1). Secure the park/turn lamp housing (3) with the 3 screws.
2. Install the park/turn lamp bulb socket (3) to the park/turn lamp housing.
3. Install the headlamp assembly (2) to the vehicle. Secure the headlamp assembly (2) with the 4 screws.
4. Install the headlamp bulb (3) to the headlamp assembly (2).
5. Turn the lock ring (4) clockwise in order to secure the headlamp bulb (3).
6. Install the grille to the vehicle. Refer to Grille Replacement in Exterior Trim.