For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (IP). Refer to Instrument Panel Assembly Replacement in Instrument Panel, Gages and Console.
2. Remove the 1 screw and the center air distributor duct (7).

### Installation Procedure

1. Install the center air distributor duct (7). Secure with the screw.
2. Install the IP. Refer to Instrument Panel Assembly Replacement in Instrument Panel, Gages and Console.