For 1990-2009 cars

1. Install the speedometer driven gear guide seal (604) and seal retainer (608), if necessary.
2. Install the speedometer driven gear (602) into the driven gear guide (603).
3. Install the speedometer driven gear guide (603) assembly into the extension housing (119).
4. Install the speedometer driven gear guide bracket (607).
5. Install the guide bracket bolt (605) and washer (606).

Tighten
Tighten the bolt to 9.5 N·m (85 lb in).

Refer to Fastener Notice .

#### Tools Required

J 36850 Transjel® Transmission Assembly Lubricant

1. Apply a thin coat of J 36850 to all speedometer driven gear components prior to assembly.
2. Install a new speedometer driven gear case lip seal into the speedometer driven gear case (2).
3. Install the speedometer driven gear (1) into the speedometer driven gear case (2).
4. Install the speedometer driven gear case (2) into the extension housing.
5. Install the speedometer guide bracket and the speedometer guide bracket bolt (1) to the extension housing.

Tighten
Tighten the speedometer guide bracket bolt (1) to 9 N·m (80 lb in).

6. Connect the speedometer cable (2) to the speedometer driven gear case.
7. Lower the vehicle.