For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster. Refer to Instrument Cluster Replacement .
2. Remove the instrument cluster lens and bezel assembly (2) from the instrument cluster (1) by releasing the 6 black plastic tabs.

Important: Do not remove the needle from the tachometer. There is no detent or flat spot on the shaft in order to indicate the correct placement.

3. Remove the following components from the instrument cluster (2):

3.1. | The 3 screws (3)

3.2. | The engine tachometer

### Installation Procedure

1. Install the engine tachometer to the instrument cluster (2). Secure the tachometer with the 3 screws (3).
2. Install the instrument cluster lens and bezel assembly (2) to the instrument cluster (1). Ensure that the plastic retaining tabs are fully engaged.
3. Install the instrument cluster. Refer to Instrument Cluster Replacement .