For 1990-2009 cars

### Removal Procedure

1. Gently pull the rear washer nozzle (3) from the rear washer nozzle mounting hole (2) above the rear door.
2. Disconnect the rear washer hose (1) from the rear washer nozzle (3).

### Installation Procedure

1. Connect the rear washer hose (1) to the rear washer nozzle (3).
2. Install the rear washer nozzle (3) to the rear washer nozzle mounting hole (2) above the rear door.