For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Place an appropriate drain pan under the engine.
3. Remove the oil pan drain plug bolt.
4. Remove the oil filter.

#### Installation Procedure

1. Install the oil filter.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the oil pan drain plug bolt.

Tighten
Tighten the oil pan drain plug bolt to 35 N·m (26 lb ft).

3. Lower the vehicle.
4. Fill the engine with oil to the appropriate mark.

Important: Oil capacity with oil and filter change is 3.7 liters (3.9 quarts)

Oil capacity with oil change only is 3.5 liters (3.7 quarts)
5. Start engine and check for leaks.