For 1990-2009 cars

### Removal Procedure

1. Remove the 2 screws which secure the license plate.
2. Remove the license plate from the front bumper fascia.

### Installation Procedure

1. Drill two 11-12 mm (7/16-1/2 in) holes approximately 20 mm (25/36 in) deep at each dimple in the front bumper fascia. Drill the holes only if you are installing the license plate for the first time.
2. Install the 2 front license plate plugs into the front bumper fascia only if you are installing the license plate for the first time.
3. Install the front license plate to the front bumper fascia. Secure the license plate with the 2 screws.