For 1990-2009 cars

#### Torque Specifications

Application | Specification
--- | ---
Metric | English
Accelerator Control Cable Adjusting Locknut | 23 N·m | 17 lb ft
Air Cleaner Assembly Bolts | 10 N·m | 89 lb in
Camshaft Position (CMP) Sensor Housing Bolts | 15 N·m | 11 lb ft
Camshaft Position (CMP) Sensor Bolt | 15 N·m | 11 lb ft
Crankshaft Position (CKP) Sensor Bolt | 10 N·m | 89 lb in
Engine Coolant Temperature (ECT) Sensor | 15 N·m | 11 lb ft
Exhaust Gas Recirculation (EGR) Valve Pipe Bolts | 15 N·m | 11 lb ft
EGR Valve Pipe Midway Bolt | 10 N·m | 89 lb in
EGR Valve Bolts | 25 N·m | 18 lb ft
Evaporative Emission (EVAP_ Canister Air Filter Fastener | 10 N·m | 89 lb in
EVAP Canister Purge Valve Bracket Bolt | 10 N·m | 89 lb in
EVAP Canister Vent Solenoid Bracket Bolt | 11 N·m | 8 lb ft
EVAP Canister Vent Valve Fastener | 10 N·m | 89 lb in
EVAP Tank Pressure Control Solenoid Valve Bracket Bolt | 25 N·m | 18 lb ft
Fuel Cut-Off Valve Fasteners | 1.6 N·m | 14 lb in
Fuel Filter Bracket Bolt | 11 N·m | 8 lb ft
Fuel Filter Bracket-to-Fuel Filter Bolt | 11 N·m | 8 lb ft
Fuel Level Vent Valve (FLVV) | 1.6 N·m | 14 lb in
Fuel Pipe Guard Nuts | 15 N·m | 11 lb ft
Fuel Pressure Regulator Bolts | 10 N·m | 89 lb in
Fuel Rail Bolts | 23 N·m | 17 lb ft
Fuel Rail Crossover Pipe Bolts | 30 N·m | 22 lb ft
Fuel Sender (fuel pump) Assembly Bolts | 5 N·m | 45 lb in
Fuel Supply Pipe and Fuel Return Pipe to Engine Bolt | 10 N·m | 89 lb in
Fuel Supply Pipe Union Bolt | 30 N·m | 22 lb ft
Fuel Tank Filler Pipe Bolts | 3.5 N·m | 30 lb in
Fuel Tank Pressure(FTP) Sensor Bolts | 1.6 N·m | 14 lb in
Fuel Tank Shield (Protector) Bolts | 50 N·m | 36 lb ft
Fuel Tank Straps Bolts | 50 N·m | 36 lb ft
Fuel Tank Vent Valve Fasteners | 3.5 N·m | 30 lb in
Heated Oxygen Sensor (HO2S) 1 | 45 N·m | 32 lb ft
HO2S 2 | 45 N·m | 32 lb ft
Idle Aie Control (IAC) Valve Fasteners | 3.5 N·m | 30 lb in
Ignition Coil Bolt | 10 N·m | 89 lb in
Ignition Coil Cover Fastener | 3 N·m | 26 lb in
Intake Collector-to-Intake Manifold Bolts and Nuts | 23 N·m | 16 lb ft
Intake Surge Tank Nuts | 23 N·m | 16 lb ft
Manifold Absolute Pressure (MAP) Sensor Fasteners | 3 N·m | 26 lb in
Negative Battery Cable-to-Negative Battery Terminal Retainer | 8 N·m | 72 lb in
PCM Bracket Bolts | 10 N·m | 89 lb in
Pressure Control Valve-to-Fuel Tank Fasteners | 3.5 N·m | 30 lb in
Spark Plugs | 25 N·m | 18 lb ft
Throttle Body Bolts and Nuts | 12 N·m | 8.5 lb ft
Throttle Position (TP) Sensor Bolts | 2.5 N·m | 22 lb in
Vehicle Speed Sensor (A/T) Bolt | 6 N·m | 54 lb in