For 1990-2009 cars

### Removal Procedure

1. Remove the front side door trim panel from the door. Refer to Front Side Door Trim Panel Replacement in Doors.
2. Remove the 4 screws which secure the front speaker (2) to the front speaker bracket (1).
3. Disconnect the front speaker electrical connector (3).
4. Remove the front speaker (2) from the vehicle.

### Installation Procedure

1. Connect the front speaker electrical connector (3).
2. Install the front speaker (2) to the front speaker bracket (1). Secure the speaker with the 4 screws.
3. Install the front side door trim panel to the door. Refer to Front Side Door Trim Panel Replacement in Doors.