For 1990-2009 cars

## Seat Cushion Release Handle Replacement 2 Door

### Removal Procedure

1. Raise the rear seat cushion (5) in order to gain access to the rear seat pull strap retaining screws (1).
2. Remove the 2 screws (1) which secure the rear seat pull strap (3).
3. Slide the pull strap (3) from the guide loop on the rear seat cushion cover and remove from the vehicle.

### Installation Procedure

1. Slide the rear seat pull strap (3) through the guide loop on the rear seat cushion cover.
2. Secure the pull strap (3) to the rear seat cushion with the 2 screws (1).
3. Lower the rear seat cushion (5).

## Seat Cushion Release Handle Replacement 4 Door

### Removal Procedure

1. Raise the rear seat cushion (2) in order to gain access to the rear seat pull strap retaining screws (4).
2. Remove the 2 screws (4) which secure the rear seat pull strap (3).
3. Slide the pull strap (3) from the guide loop on the rear seat cushion cover and remove from the vehicle.

### Installation Procedure

1. Slide the rear seat pull strap (3) through the guide loop on the rear seat cushion cover.
2. Secure the pull strap (3) to the rear seat cushion with the 2 screws (4).
3. Lower the rear seat cushion (2).