For 1990-2009 cars

### Removal Procedure

1. Remove the screw which secures the front side door inside handle (1).
2. Slide the inside handle (1) forward in order to release the retaining tabs which secure the handle to the door.
3. Open the front side door inside handle rod retainer and remove the front side door inside handle rod from the inside handle (1).
4. Remove the inside handle (1) from the vehicle.

### Installation Procedure

1. Install the front side door inside handle rod to the front side door inside handle (1). Secure the rod to the handle by closing the front side door inside handle rod retainer.
2. Install the inside handle (1) to the door by sliding rearward to engage the retaining tabs. Secure the handle with the screw.