For 1990-2009 cars

## Rear Seat Back Cushion Cover Replacement 4 Door

### Removal Procedure

1. Remove the rear seatback. Refer to Rear Seat Back Replacement .
2. Unscrew the 2 rear seatback lock knobs counterclockwise.
3. Remove the rear seatback lock knobs from the seat.
4. Unzip the rear seatback cover.
5. Slide the rear seatback cover off of the seatback frame.

### Installation Procedure

1. Slide the rear seatback cover over the seatback frame.
2. Zip the cover closed.
3. Install the 2 rear seatback lock knobs to the seatback by screwing the lock knobs clockwise.
4. Install the rear seatback. Refer to Rear Seat Back Replacement .

## Rear Seat Back Cushion Cover Replacement 50/50 Split

### Removal Procedure

1. Remove the rear seatback. Refer to Rear Seat Latch Replacement .
2. Unscrew the rear seatback lock knob counterclockwise. Remove the rear seatback lock knob from the seatback.
3. Unzip the seatback cover. Slide the seatback cover off the seatback frame.

### Installation Procedure

1. Slide the rear seatback cover onto the seatback frame. Zip the cover closed.
2. Install the rear seatback lock knob to the seatback. Screw the rear seatback lock knob clockwise in order to secure the rear seatback lock knob to the seatback.
3. Install the rear seatback. Refer to Rear Seat Latch Replacement .