For 1990-2009 cars

Caution: Handle the piston carefully. Worn piston rings are sharp and may cause bodily injury.

1. Disassemble the piston rings. Use a suitable tool in order to expand the rings. The piston rings must not be reused.
2. Using a screwdriver, remove the piston snap rings (1).
3. Carefully remove the piston pin from the piston and connecting rod.

• | The piston and pin are a matched set.

• | Arrange the pistons, pins, rings, connecting rods and bearings in correct order.