For 1990-2009 cars

### Removal Procedure

1. Remove the following components from the instrument panel:

1.1. | The 3 screws (2)

1.2. | The IP steering column opening trim plate (1)

2. Release the upper and lower retaining tabs behind the instrument panel which secure the rear window wiper/washer switch (2).
3. Slide the rear window wiper/washer switch (2) from the instrument panel in order to disconnect the electrical connector.
4. Disconnect the rear window wiper/washer switch electrical connector.
5. Remove the rear window wiper/washer switch (2) from the vehicle.

### Installation Procedure

1. Connect the rear window wiper/washer switch electrical connector.
2. Install the rear window wiper/washer switch (2) to instrument panel. Ensure that the retaining tabs are fully engaged.
3. Install the IP steering column opening trim plate (1) to the instrument panel. Secure the trim plate with the 3 screws (2).