For 1990-2009 cars

1. Remove the parking pawl plate bolts.
2. Remove the parking pawl plate.
3. Remove the following components from the transmission case:

• | The parking pawl torsion spring

• | The pivot pin

• | The parking pawl (2)

4. Remove the parking pawl rod (1) from the manual shift shaft.
5. Remove the manual lever hub protection sleeve (1) from the manual detent lever hub (2) using a hammer and a chisel.
6. Remove the manual detent lever hub roll pin using a standard drift punch and a hammer.
7. Remove the following components from the transmission case:

• | The manual shaft (2)

• | The manual detent lever (1)

8. Remove the manual shaft oil seals (1) from both sides of the transmission case (2) using a flathead screwdriver.