For 1990-2009 cars

### Removal Procedure

1. Remove the compressor relay (2) from the fuse box mounting bracket.
2. Remove the rubber sleeve from the compressor relay.
3. Disconnect the compressor relay from the electrical connector.

### Installation Procedure

1. Connect the compressor relay (2) to the electrical connector.

Important: If the rubber sleeve is not correctly installed water and other contaminant intrusion may result and affect proper A/C operation.

2. Install the rubber sleeve to the compressor relay.
3. Install the compressor relay to the mounting bracket.