For 1990-2009 cars

### Circuit Description

The DTC P0107 Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage diagnostic monitors the MAP sensor response to pressure changes in the intake manifold. The pressure changes occur based on engine load and the throttle valve opening. The MAP sensor has the following circuits:

• | A 5-volt reference circuit

• | A low reference circuit

• | A signal circuit

The powertrain control module (PCM) supplies 5 volts to the MAP sensor on the 5 volt reference circuit. The PCM also provides a ground on the low reference circuit. The PCM receives a low voltage on the signal circuit when manifold vacuum is high at idle or deceleration. The PCM receives a high voltage when manifold vacuum is low at wide open throttle (WOT) or when the ignition is ON and the engine is OFF. The PCM monitors the MAP sensor signal for voltage outside of the normal range and sets a DTC P0107 when the voltage is unusually low.

Engine Condition | MAP kPa | MAP Signal Voltage | Manifold Vacuum
--- | --- | --- | ---
Idle | Low | Low | High
Deceleration | Low | Low | High
Ignition ON, Engine OFF | High | High | Zero
Wide-Open Throttle | High | High | Low

### Conditions for Running the DTC

• | Barometric pressure is more than 75 kPa.

• | The intake air temperature (IAT) is more than -10°C (14°F).

• | The engine coolant temperature (ECT) is more than 80°C (176°F).

• | Vehicle speed is detected

• | The throttle valve opening is more than a specified value.

### Conditions for Setting the DTC

The MAP sensor signal is less than 1.0 volt for 40 seconds or more.

### Action Taken When the DTC Sets

• | The PCM illuminates the malfunction indicator lamp (MIL) after 2 consecutive ignition cycles in which the diagnostic runs with the fault active.

• | The PCM records the operating conditions at the time the diagnostic fails. This information is stored in the Freeze Frame buffer.

### Conditions for Clearing the MIL/DTC

• | The MIL turns OFF after 3 consecutively passing trips without a fault present.

• | A history DTC clears after 40 consecutive warm-up cycles without a fault.

• | Perform the scan tool Clear DTC Information function.

### Diagnostic Aids

If a DTC P0107 is intermittent, driving the vehicle under the following conditions can verify whether the fault is present. Perform the scan tool Clear DTC Information function. Road test the vehicle while monitoring the DTC P0107 diagnostic on the scan tool under the Not Ran Since Code Cleared selection in the DTC Information menu. If DTC P0107 appears in the Not Ran Since Code Cleared list, the P0107 diagnostic has not yet run. When DTC P0107 does not appear in the Not Ran Since Code Cleared list, the DTC P0107 diagnostic has run. If the MIL is NOT illuminated, and there is no Pending DTC Status in DTC Information, the DTC P0107 diagnostic has passed. The DTCs MUST be cleared in order to view the Current Status of the Not Ran Since Code Cleared list. DO NOT forget that the Not Ran Since Code Cleared list only indicates that the test has run, not whether the test passed or failed. The DTC Information screen must be checked for Current or Pending status in order to determine the outcome of the diagnostic test involved.

An intermittent malfunction may be caused by a fault in the MAP sensor circuit. Inspect the wiring harness and the components for an intermittent condition. Refer to Intermittent Conditions .

If the DTC P0107 cannot be duplicated, the information included in the Freeze Frame data can be useful in determining the vehicle operating conditions when the DTC was first set.

### Test Description

The numbers below refer to the step numbers in the diagnostic table:

1. The Diagnostic System Check-Engine Controls prompts the technician to complete some basic checks and store the Freeze Frame data on the scan tool if applicable. This creates an electronic copy of the data taken when the fault occurred. The information is then stored in the scan tool for later reference.

2. Clearing the DTCs by removing the DOME fuse also clears the PCM long term memory. Using the scan tool to clear DTCs leaves the long term memory active. DTC emitting diagnostics may not run to completion as expected unless the long term memory is cleared. Removal of the DOME fuse also clears the time display of the radio.

3. This step checks for the correct reference circuit voltage. The scan tool display of MAP sensor voltage will indicate more than 5 volts with an open in the sensor input circuit. This is caused by the scan tool software and should be considered normal.

4. This step checks the integrity of the MAP sensor signal circuit. The scan tool MAP sensor voltage display will indicate more than 5 volts with the signal and reference circuits jumpered together. This is caused by the scan tool software and should be considered normal. The actual measured voltage at the PCM is only 5 volts.

5. The 5 volt reference circuit is shared internally in the PCM with the fuel tank pressure (FTP) sensor. Be sure to inspect the FTP sensor reference circuit for a short to ground.

6. Clearing the DTCs by removing the DOME fuse also clears the PCM long term memory. Using the scan tool to clear DTCs leaves the long term memory active. DTC emitting diagnostics may not run to completion as expected unless the long term memory is cleared. Removal of the DOME fuse also clears the time display of the radio. The DTC P0107 diagnostic can be monitored on the scan tool under the Not Ran Since Code Cleared selection in the DTC Information menu. If a DTC P0107 appears in the Not Ran Since Code Cleared list, the DTC P0107 diagnostic has not yet run. When the DTC P0107 does not appear in the Not Ran Since Code Cleared list, the DTC P0107 diagnostic has run. If the MIL is NOT illuminated, and there is no Pending DTC Status in DTC Information, the DTC P0107 diagnostic has passed. The DTCs MUST be cleared in order to view the Current Status of the Not Ran Since Code Cleared list. DO NOT forget that the Not Ran Since Code Cleared list only indicates that the test has run, not whether the test passed or failed. The DTC Information screen must be checked for Current or Pending status, in order to determine the outcome of the diagnostic test involved.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
Schematic Reference: Engine Controls Schematics
1 | Did you perform the Diagnostic System Check-Engine Controls? | -- | Go to Step 2 | Go to Diagnostic System Check - Engine Controls
2 | Is there a DTC P0122 and DTC P0452 also set? | -- | Go to Step 8 | Go to Step 3
3 |

1. Turn ON the ignition, leaving the engine OFF.
2. Install a scan tool.
3. Select the MAP sensor parameter on the scan tool.

Is the MAP sensor display at or below the specified value?

1.0 V

Go to Step 5

Go to Step 4

4 |

1. Turn OFF the ignition.
2. Remove the DOME fuse for 30 seconds.
3. Install the DOME fuse.
4. Reset the radio clock time. Refer to Radio/Audio System Description and Operation in Entertainment.
5. Start the engine.
6. Operate the vehicle within the Freeze Frame conditions as noted.
7. Observe the MAP sensor voltage on the scan tool.

Did a DTC P0107 set or did the MAP sensor voltage stay below the specified value?

1.0 V

Go to Step 5

Go to Diagnostic Aids

5 |

1. Turn OFF the ignition.
2. Disconnect the MAP sensor electrical connector.
3. Turn ON the ignition, leaving the engine OFF.
4. Measure the voltage from the 5 volt reference circuit to ground, harness side with a DMM.

Is the voltage near the specified value?

5.0 V

Go to Step 6

Go to Step 9

6 |

1. Turn OFF the ignition.
2. Jumper the 5 volt reference circuit of the MAP sensor to the MAP sensor signal circuit.
3. Turn ON the ignition, leaving the engine OFF.
4. Observe the MAP sensor voltage on the scan tool.

Is the scan tool voltage within the specified value?

5.0-6.0 V

Go to Step 7

Go to Step 10

7 | Replace the MAP sensor. Refer to Manifold Absolute Pressure Sensor Replacement . Did you complete the replacement? | -- | Go to Step 13 | --
8 |

1. Inspect for a short to ground in the 5 volt reference circuit.
2. Repair as necessary. Refer to Wiring Repairs in Wiring Systems.

Did you find and correct the condition?

--

Go to Step 13

Go to Step 12

9 |

1. Check for an open in the 5 volt reference circuit between the PCM and the MAP sensor.
2. Repair as necessary. Refer to Wiring Repairs in Wiring Systems.

Did you find and correct the condition?

--

Go to Step 13

Go to Step 11

10 |

1. Check for an open or a short to ground in the MAP sensor signal circuit between the PCM and the MAP sensor.
2. Repair as necessary. Refer to Wiring Repairs in Wiring Systems.

Did you find and correct the condition?

--

Go to Step 13

Go to Step 11

11 |

1. Inspect the PCM and the MAP sensor electrical connectors for faulty terminal contact. Refer to Testing for Intermittent Conditions and Poor Connections in Wiring Systems.
2. Repair as necessary.

Did you find and correct the condition?

--

Go to Step 13

Go to Step 12

12 | Important: The replacement PCM must be programmed. Replace the PCM. Refer to Powertrain Control Module Replacement . Did you complete the replacement? | -- | Go to Step 13 | --
13 |

1. Turn OFF the ignition.
2. Remove the DOME fuse for 30 seconds.
3. Install the DOME fuse.
4. Reset the radio clock time. Refer to Radio/Audio System Description and Operation in Entertainment.
5. Start the engine.
6. Operate the vehicle within the Conditions for Running the DTC as specified in the supporting text or until the DTC P0107 diagnostic test has run.

Does the DTC run and pass?

--

Go to Step 14

Go to Step 2

14 | With a scan tool, observe the stored information, Capture Info. Does the scan tool display any DTCs that you have not diagnosed? | -- | Go to Diagnostic Trouble Code (DTC) List | System OK