For 1990-2009 cars

### Removal Procedure

1. Grasp the lower corner of the windshield reveal molding (1) by hand and slowly pull the reveal molding away from the windshield (4).
2. If the windshield reveal molding will not release, use a utility knife in order to cut around the windshield in order to remove the windshield reveal molding.
3. Remove the windshield reveal molding.

### Installation Procedure

1. Trim the windshield reveal molding (1), as needed, in order to fit the molding in the cavity around the windshield (4).
2. Install the windshield reveal molding (1). Refer to .

Starting from the center, firmly press the windshield reveal molding (1) into place.