For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Distance from the Brake Pedal to the Bulkhead Without Pressure on the Brake Pedal | 175-185 mm with 0 kg or 0 N of force | 6.90-7.30 in with 0 lbs of force
Distance from the Brake Pedal to the Bulkhead With Pressure on the Brake Pedal | 100-120 mm with 30 kg or 294 N of force | 3.94-4.72 in with 66 lbs of force
Push Rod Clevis Length | 109.5-110.5 mm | 4.31-4.35 in
Stoplamp Switch-to-Brake Pedal Clearance | 1.5-2.0 mm | 0.06-0.08 in
Distance from the Booster Piston Rod to the Mating Surface of the Booster:

- 1.6L Non-ABS

9.40-9.62 mm

0.370-0.378 in