For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Exterior Lights Circuit Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Lighting Systems
2 | Verify that the license plate and tail lamps are inoperative. Are the license plate and tail lamps inoperative? | Go to Step 3 | Go to Testing for Intermittent Conditions and Poor Connections
3 |

1. Disconnect C207. Refer to Lighting Systems Components .
2. Turn the light switch to the ON position.
3. Test for battery voltage at terminal 6 of C207.

Is battery voltage present?

Go to Step 5

Go to Step 4

4 | Repair the open in the RED/YEL wire between C207 and S217. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 8 | --
5 |

1. Connect C207.
2. Disconnect C213. Refer to Lighting Systems Components .
3. Turn the light switch to the ON position.
4. Test for battery voltage at terminal 2 of C213.

Is battery voltage present?

Go to Step 7

Go to Step 6

6 | Repair the open in the RED/YEL wire between C207 and C213. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 8 | --
7 | Repair the open in the RED/YEL wire between C213 and S305. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 8 | --
8 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3