For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Place a reference mark (3) on the pinion flange yoke and the differential pinion flange (2).
3. Remove the 4 bolts (1) and the 4 nuts (4) and lock washers.
4. Remove the mid shaft bearing support bolts (1, 2).
5. Remove the sliding yoke (1) and the two piece propeller shaft assembly from the transmission.
6. Inspect the shaft for dents or other damage. Replace the shaft if the shaft is damaged.
7. Inspect the universal joints for smooth pivoting. If the universal joints bind or appear tight replace the universal joints as assembled.
8. Inspect the sliding yoke splines (1) for excessive wear or damage. If the splines (1) appear worn or rounded, replace the sliding yoke (3).
9. Inspect the sliding yoke for the following:

• | Scoring

• | Burrs

• | Other damage

• | If the sliding yoke surface appears scored or rough, replace the sliding yoke.

10. Inspect the pinion flange yoke for the following:

• | Cracks

• | Distortion

• | Other damage

• | If the pinion flange yoke appears damaged or distorted, replace the pinion flange yoke.

### Installation Procedure

1. Install the sliding yoke (1) into the transmission with the two piece propeller shaft assembly.
2. Ensure that the sliding yoke splines are lubricated.
3. Align the mid shaft bearing support 90 degrees to the propeller shaft center lines.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the mid shaft bearing support bolts (1, 2).

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

5. Install the pinion flange yoke (4) to the differential pinion flange (3) with the reference marks (2). Secure the pinion flange yoke with 4 bolts and 4 nuts and lock washers.

Tighten
Tighten the propeller shaft bolts and nuts to 50 N·m (37 lb ft).

6. Lower the vehicle.