For 1990-2009 cars

### Removal Procedure

1. Pull out the instrument panel compartment while pushing in the right and left stoppers.
2. Disconnect the blower motor resistor electrical connector.
3. Remove 1 screw (1) from the blower case.
4. Remove 1 blower motor resistor (2) from the blower case.

### Installation Procedure

1. Install the blower motor resistor (2) to the blower case.
2. Secure the resistor with 1 screw (1).
3. Connect the blower motor resistor electrical connector.
4. Close the instrument panel compartment.