For 1990-2009 cars

### Removal Procedure

1. Remove the front side door water deflector. Refer to Front Side Door Water Deflector Replacement .
2. Open the front side door lock cylinder rod retainer and remove the front side door lock cylinder rod from the front side door lock cylinder.
3. Remove the front side door lock cylinder retainer which secures the lock cylinder.
4. Remove the front side door lock cylinder from the door.

### Installation Procedure

1. Install the front side door lock cylinder to the door. Secure the lock cylinder with the front side door lock cylinder retainer.
2. Install the front side door lock cylinder rod to the lock cylinder. Secure the rod by closing the front side door lock cylinder rod retainer.
3. Install the front side door water deflector. Refer to Front Side Door Water Deflector Replacement .