For 1990-2009 cars

### Removal Procedure

1. Remove the folding top from the vehicle. Refer to Folding Top Material Replacement .
2. Remove the garnish moldings.
3. Remove the 4 screws and the top rear bow.

### Installation Procedure

1. Install the top rear bow to the vehicle. Secure the top rear bow with the 4 screws.
2. Install the garnish moldings.
3. Install the folding top to the vehicle. Refer to Folding Top Material Replacement .