For 1990-2009 cars

## Rear Seat Cushion Cover Replacement 2 Door

### Removal Procedure

1. Lift up the rear seat cushion (1).
2. Remove the rear seat pull strap (2) from the guide loop (3) on the rear seat cushion cover (1).
3. Release the lace (1) which secures the seat cushion cover (2) to the rear seat cushion frame.
4. Remove the seat cushion cover (1) from the seat cushion pad (2) and frame.

### Installation Procedure

1. Install the rear seat cushion cover (1) to the rear seat cushion pad (2) and frame.
2. Secure the seat cushion cover (2) to the rear seat cushion frame with the lace (1).
3. Install the rear seat pull strap (2) to the guide loop (3) on the rear seat cushion cover (1).
4. Lower the rear seat cushion (1).

## Rear Seat Cushion Cover Replacement 4 Door

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Remove the rear seat pull strap (1) from the guide loop (2) on the rear seat cushion cover (4).
3. Release the lace (3) which secures the seat cushion cover (4) to the rear seat cushion frame (5).
4. Remove the seat cushion cover (1) from the seat cushion pad (2) and frame.

### Installation Procedure

1. Install the rear seat cushion cover (1) to the rear seat cushion pad (2) and frame.
2. Secure the seat cushion cover (4) to the rear seat cushion frame (5) with the lace (3).
3. Install the rear seat pull strap (1) to the guide loop (2) on the rear seat cushion cover (4).
4. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .