For 1990-2009 cars

### Removal Procedure

1. Remove the following components from the vehicle:

1.1. | The 3 plastic retainers

1.2. | The rear side door sill trim plate

2. Turn the retainer counterclockwise in order to unlock the jack storage cover (1).
3. Remove the jack storage cover (1) from the vehicle.
4. Remove the lug wrench (3) and the jack handle (4) from the rear quarter lower trim panel (2).
5. Fold the rear seat back cushion forward in order to gain the necessary clearance to remove the rear quarter lower trim panel.
6. Pull and remove the rear quarter lower trim panel (2) from the vehicle by disengaging the plastic retainers.

### Installation Procedure

1. Install the rear quarter lower trim panel (2) to the vehicle. Press the panel into place ensuring that the plastic retainers are fully engaged.
2. Fold the rear seat back cushion to the upright position.
3. Install the lug wrench (3) and the jack handle (4) to the rear quarter lower trim panel (2).
4. Install the jack storage cover (1) to the vehicle and turn the retainer clockwise in order to secure the jack storage cover (1).
5. Install the rear side door sill trim plate to the vehicle. Secure the trim plate with the 3 plastic retainers.