For 1990-2009 cars

### Removal Procedure

1. Remove the IP cluster trim plate. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement in Instrument Panel, Gages and Console.
2. Using a taped flat bladed tool, gently pry the cruise control switch from the instrument panel.
3. Disconnect the cruise control switch electrical connector.
4. Remove the switch from the vehicle.

### Installation Procedure

1. Connect the cruise control switch electrical connector.
2. Install the cruise control switch to the instrument panel. Ensure that the retaining tabs are fully engaged.
3. Install the IP cluster trim plate. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement in Instrument Panel, Gages and Console.