For 1990-2009 cars

### Removal Procedure

1. Remove the nut (2) which secures the rear door strut (1) to the rear door.
2. Remove the nut (2) which secures the rear door strut (1) to the rear door opening.
3. Remove the rear door strut (1) from the vehicle.

### Installation Procedure

1. Install the rear door strut (1) to the rear door opening. Secure the strut with the nut (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the rear door strut (1) to the rear door. Secure the strut with the nut (2).

Tighten
Tighten the rear door strut nuts to 15 N·m (11 lb ft).