For 1990-2009 cars

## Rear Door Weatherstrip Replacement 4 Door

### Removal Procedure

Remove the rear door opening weatherstrip from the vehicle by pulling the weatherstrip from the pinch weld flange.

### Installation Procedure

Install the rear door opening weatherstrip to the pinch weld flange. Ensure that the weatherstrip is fully seated on the flange.

## Rear Door Weatherstrip Replacement 2 Door

### Removal Procedure

Remove the endgate opening weatherstrip from the vehicle by pulling the weatherstrip from the pinch weld flange.

### Installation Procedure

Install the endgate opening weatherstrip to the pinch weld flange. Ensure that the weatherstrip is fully seated on the flange.