For 1990-2009 cars

## Body Side Lower Front Molding Bracket Replacement LT Models

### Removal Procedure

1. Remove the rear body side lower molding. Refer to Molding Replacement - Rear Body Side Lower .
2. Drill out and remove the 3 rivets (3) that retain the body side lower molding bracket (1).
3. Remove the body side lower molding bracket (1) from the quarter panel (2).

### Installation Procedure

1. Install the body side lower molding bracket (1) to the quarter panel (2). Secure the bracket with 3 rivets (3).
2. Install the rear body side lower molding. Refer to Molding Replacement - Rear Body Side Lower .