For 1990-2009 cars

### Removal Procedure

1. Disconnect the CKP sensor electrical connector (2).
2. Remove the bolt (3) from the CKP sensor and the oil pan.
3. Remove the CKP sensor (1) from the oil pan.

### Installation Procedure

1. Install the CKP sensor (1) to the oil pan.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Secure the CKP sensor to the oil pan with one bolt (3).

Tighten
Tighten the sensor bolt to 15 N·m (11 lb ft).

3. Connect the CKP sensor electrical connector (2).