For 1990-2009 cars

### Removal Procedure

1. Push in the folding top latch buttons (2).
2. Pull the latch (1) back.
3. Unhook the latch (1) from the front top bow.
4. Lift the front top bow.
5. Unsnap the folding top material (3, 4) from the front top bow (1, 2).
6. Unsnap the tension straps (1) from the roof rails in order to pull the straps out of the plastic loops (2).
7. Remove the 4 front top bow screws.
8. Remove the front top bow from the vehicle.

### Installation Procedure

1. Install the front top bow to the vehicle. Secure the front top bow with the 4 screws.
2. Pull the tension straps (1) through the plastic loops (2) in order to snap the tension straps (1) to the roof rails.
3. Snap the folding top material (3, 4) to the front top bow (1, 2).
4. Move the front top bow (1, 2) forward.
5. Hook the front top bow to the folding top latches (1).
6. Push the latches (1) down until the latches click into place.