For 1990-2009 cars

Figure 1: |

#### Two Wheel Drive Front Suspension Components

(1) | Body
(2) | Strut
(3) | Coil Spring
(4) | Control Arm
(5) | Bump Stopper
(6) | Ball Stud
(7) | Wheel
(8) | Wheel Hub
(9) | Wheel Bearing
(10) | Steering Knuckle

Figure 2: |

#### Four Wheel Drive Front Suspension Components

(1) | Body
(2) | Strut
(3) | Coil Spring
(4) | Control Arm
(5) | Bump Stopper
(6) | Drive Axle
(7) | Ball Stud
(8) | Wheel
(9) | Wheel Hub
(10) | Wheel Bearing
(11) | Steering Knuckle

The front suspension is laterally independent. The front suspension uses the following components:

• | Struts

• | Separate coil springs

A strut support anchors the upper end of each strut to the body. A rubber mount isolates each strut and its strut support.

The lower end of the strut is connected to the upper end of a steering knuckle. The lower end of the steering knuckle is attached to a ball stud. The ball stud is part of a unit with a control arm.

Movement of the steering wheel is transmitted to the tie rod end and then to the knuckle. This movement causes the wheel to turn.